영  문   규  격  서

COMMODITY DESCRIPTION

H.S. No.	Item No.	Description	Unit	Quantity
		Hi/Lo Profile Rocker (Model ROCAA220S)	Set	1

Manufacturer:  Stovall Life Science, Inc., U.S.A.

A. Feature:

- This light weight, low profile rocker unit is designed for versatility.

- It operates on bench tops, in high humidity or dry incubators, in high

temperature ovens (to 60°C) and in refrigerated units (to 0°C).

Typical applications are:

•Staining and destaining gels

•Northern and Southern Hybridizations

•Western blotting and rinsing membraines

•Cell culture incubation

•Phage elution, Amplification of cDNA libraries

- The easily adjustable speed and platform pitch controls provide a wide

range of agitation conditions: from extremely gentle to vigorous.

- The gentle agitation conditions are excellent for cell cultures.

B. Specification:

1. Hi/Lo Profile Rocker, 230V                           1 Set

- Overall Dimensions: 13 3/4" × 15 3/4" × 1 3/4" H

3 3/4 " Motor Module Height

- Weight: 16 lbs

- Ambient Temp. Operation:  0° C to 60° C

- Electrical: 230 Volt AC, 50/60Hz, 1 Amp.

- Motor:  24 Volt Permanent Magnet DC

- Speed:  0 - 60 rpm

- US Patent # 5423603