영  문   규  격  서

COMMODITY DESCRIPTION

H.S. No.	Item No.	Description	Unit	Quantity
8479.82-2000		Ultrasonic Processor (Model VCX-130)	Set	1

Manufacturer:  Sonics & Materials, Inc., U.S.A.

A. Feature:

1. Extremely versatile, it safely process a wide range of organic and inorganic

materials - from microliters to liters. Typical applications include: sample

preparation, cell lysing, disaggregation, partical size reduction, soil testing,

acceleration of chemical reactions, defoaming and atomization.

2. Digital acuracy and repeatability eliminates the need for constant attention,

and assures adherence to the most exacting protocol.

3. To give you complete freedom to focus on what's important and guaranty                   consistent and accurate reproducibility, the unit combines our proprietary              automatic tuning control with power-on-demand technology. Feedback from the             probe is continuously evaluated, and frequency and power automatically adjusted          to ensure optimum ultrasonic delivery

B. Specification:

1.  Ultrasonic Processor, 130 Watt               1 Set

1) Power Supply

․ Net Power Output: 130 Watt

․ Frequency: 20kHz

2) Converter

․ Type:  Piezoelectric-PZT-Lead

Zirconate Titanate Crystals

․ Diameter: 32mm

․ Length: 146mm

․ Weight: 340g

․ Cable Length: 1.5m

3) Standard Probe

․ Tip Diameter: 3mm

․ Processing Capability: 250ul - 10ml

․ Length: 138mm

․ Titanium Alloy: TI-6AL-4V

4) Power: 220V, 50/60Hz

Accessories:

1) 6mm Stepped Microtip            1 Ea

2) Sound Abating Enclosure         1 Ea

3) Heavy Duty Converter Clamp      1 Ea