영  문   규  격  서

COMMODITY DESCRIPTION

H.S. No.	Item No.	Description	Unit	Quantity
8479.82-2000		Ultrasonic Processor (Model VCX-1500)	Set	1

Manufacturer:  Sonics & Materials, Inc., U.S.A.

A. Feature:

1. The unit can be used by itself or with the optional high volume continuous

flow cell. When used in conjunction with the flow cell, throughput rate is

typically 100 liters/hour - variables being viscosity and desired degree

of processing.

2. The flow cell is recommended for the treatment of low viscosity samples which

do not require extended exposure to ultrasonics.

3. Designed primarily for dispersing and homogenizing. For optimum performance,

when working on a flow through basis, premix the sample with a mechanical

mixer or a stirrer. Easily disassembled for inspection and cleaning.

B. Specification:

1.  Ultrasonic Processor, 1500 Watt                 1 Set

1) Power Supply

․ Net Power Output: 1500 Watt

․ Frequency: 20kHz

2) Air Cooled Converter

․ Type:  Model CV 294. Piezoelectric-PZT-Lead

Zirconate Titanate Crystals

․ Diameter: 76.2mm

․ Length: 158.7mm

․ Weight: 900g

․ Cable Length: 3.0m

3) Booster:  BHNVC21 - Increases the amplitude by a factor of 2

4) Standard Probe

․ Tip Diameter: 25mm

․ Processing Capability: 4 liters up to 20 liter

when used with a 1" (25 mm) solid 181⁄2" (470 mm) long probe

․ Length: 254mm

․ Titanium Alloy: TI-6AL-4V

5) Power: 220V, 50/60Hz

Accessories:

1) High Volume Continuous Flow Cell  with Probe      1 Ea

2) Sound Abating Enclosure                           1 Ea