국  문   규  격  서

COMMODITY DESCRIPTION

H.S. No.	Item No.	Description	Unit	Quantity
8479.82-2000		초음파 파쇄기 (Model VCX-750)	대	1

제조사:  Sonics & Materials, Inc., U.S.A.

A. 특성:

1. 자동 튜닝 및 주파수 조정으로 전원공급기를 계속적으로 조정해야할 필요성을 없애준다

2. 본 기기는 유기물과 무기물을 광벙위하게 마이크로리터 (㎕)에서 리터(ℓ)의 용량으로           지극히 다양하게 그리고 안전하게 처리할 수 있다. 대표적인 용도는 다음과 같다. 샘플          준비작업, 세포용해, 집산(集散), 입자크기감소작업, 토양시험, 화학작용의 가속화, 거품         제거 및 분무작용 등.

3. 디지털의 정확성과 재현성은 계속인 주의를 요하는 작업을 줄여주며 가장 엄격하게 적용         되는 프로토콜에 대한 신뢰성을 확보할 수 있다.

4. 샘플이 미리 입력한 제한 온도에 도달할 경우 초음파분사를 종료시키므로써 샘플에 위험         한 과열현상를 막아주므로 실험진행의 안정을 보장한다. 1℃에서 100℃까지 조정 및 감지         가 가능하다. (선택 사양인 온도 프로브(탐침)를 사용할 경우)

5. 본 기기는 복잡한 프로토콜의 반복적 사용이 가능하며, 매우 편리하게 10개의 프로그램까         지 저장할 수 있다. 앞으로의 사용을 위해 저장할 수 있으며, 확인과 변경을 위해서 다시         불러낼 수 있다

6. 작업시간을 1초에서 10시간까지 조정할 수 있다

B. 제원:

1.  초음파 파쇄기, 750 Watt               1 Set

1) 전원공급기  :  - Net Power Output: 750 Watt

- Frequency: 20kHz

2) 변환기   :     - Type: Piezoelectric-PZT-Lead Zirconate Titanate Crystals

- Diameter: 63.5mm

- Length: 183mm

- Weight: 900g

3) 표준프로브(검침): - Tip Diameter: 13mm threaded end with replaceable tip.

- Processing Capability: 10ml to 250ml

- Length: 136mm

- Weight: 340g

- Titanium Alloy: TI-6AL-4V

4)  전원: 220V, 50/60Hz

Accessories:

1) Tapered Microtip, 3mm, 1-10ml             1 Ea

2) Sound Abating Enclosure                   1 Ea

3) Heavy Duty Clamp and Stand                1 Ea