영  문   규  격  서

COMMODITY DESCRIPTION

H.S. No.	Item No.	Description	Unit	Quantity
9027.90-9190		UV Transilluminator	Set	1

A. Feature:

1. Specially designed to satisfy most analytical requirements and electrophoresis

gel preparation (agarose or polyacrylamide).

2. The unit is characterized by its powerful illumination and its capacity to

detect bands at a very low threshold. A UV intensity selector with two positions

(100% and 70%) allows work to be carried out in two ways: 100% reading of gels          and 70% preparation.

3. The 312 wavelength provides minimal risks of photodamage, photonicking and               photodimerization in applications such as: cloning and chromosomal mapping.

B. Specification:

1. ECX-20.M   UV Transilluminator                     1 Ea

- Filter Size: 20 x 20cm

- UV Wavelength: 312nm

- UV Tubes: 6 x 8 Watt 312nm Tubes

- UV Intensity: 10000uW/㎠

- UV Safety Screen (Cover)

- Dual Intensity Selector (100%/70%)

- 240V voltage, 50/60Hz